# MiktoTik Configuration Steps
### We need to configure MikroTik servers for two end use cases - PPPoE or HotSpot. here are the steps to achieve them through MikroTik's REST API facility. Use the `MiktoTik (EasyFi)` Postman collection for this.
#### Authors: Bhushan, Hari, Khushal
#### Date: 20250209


### General Notes:

Private IP series has been allocated for doing carrier-grade NAT = 100.64.0.0/10

PPPoE:
- PPPoE user master subnet = 100.64.0.0/16
- pppoe_ip_subnet: 100.64.0.0/24 = if user is under 256
- pppoe_ip_subnet: 100.64.0.0/23 = if user is under 512
- pppoe_ip_subnet: 100.64.0.0/22 = if user is under 1024
- pppoe_ip_subnet: 100.64.0.0/21 = if user is under 2048
- PPPoE deactivated user master subnet = 10.0.0.0/16

HotSpot
- HotSpot user master subnet = 100.65.0.0/16
- hotspot_ip_subnet: 100.65.0.0/24 = if user is under 256
- hotspot_ip_subnet: 100.65.0.0/23 = if user is under 512
- hotspot_ip_subnet: 100.65.0.0/22 = if user is under 1024
- hotspot_ip_subnet: 100.65.0.0/21 = if user is under 2048

---

## Steps for HotSpot

### 1. Interface 
- Enlist the available interfaces.
- Select the first one that has field `"running"` set to `"false"`, and pick its `".id"`.
- Rename it to `"easyfi-hs"` by its `".id"`.

### 2. Create a VLAN
Create a VLAN with the following config:
```json
{
    "name": "easyfi-vlan-<vlan_id>",
    "interface": "easyfi-hs",  // The name that was given in the previous step.
    "vlan-id": "<vlan_id>",  // From the config received on the portal.
    "disabled": "no"
}
```

### 3. Add a new IP Address to the VLAN interface
```json
{
    "address": "<hotspot_ip_subnet>",  // Refer to the general notes.
    "interface": "easyfi-vlan-<vlan_id>",  // Same as the 'name' given in the previous step. 
    "disabled": "no"
}
```

### 4. Add a New IP Pool for HotSpot Users
```json
{
    "name": "easyfi-hs-pool-<vlan_id>",
    "ranges": "<hotspot_ip_subnet>"  // Refer to the general notes.
}
```

### 5. Add a New HotSpot Profile
```json
{
    "dns-name": "hs01.easyfi.net.in",
    "hotspot-address": "100.65.0.1",  // First from the subnet. Refer to the general notes.
    "html-directory": "hotspot",
    "html-directory-override": "",
    "http-cookie-lifetime": "3d",
    "http-proxy": "0.0.0.0:0",
    "install-hotspot-queue": "false",
    "login-by": "cookie,http-chap",
    "name": "hs01.easyfi.net.in",
    "split-user-domain": "false",
    "use-radius": "true",
    "nas-port-type": "wireless-802.11",
    "radius-accounting": "true",
    "radius-default-domain": "",
    "radius-interim-update": "received",
    "radius-location-id": "",
    "radius-location-name": "",
    "radius-mac-format": "XX:XX:XX:XX:XX:XX"
}
```

### 6. Add a New HotSpot Server
```json
{
    "address-pool": "easyfi-hs-pool-<vlan_id>", // Same as the name given when creating the pool.
    "addresses-per-mac": "2",
    "idle-timeout": "5m",
    "interface": "easyfi-vlan-<vlan_id>", // Same as the 'name' given when creating the VLAN.
    "keepalive-timeout": "none",
    "login-timeout": "none",
    "name": "hs01.easyfi.net.in",
    "profile": "hs01.easyfi.net.in",
    "disabled": "false"
}
```

### 7. Add a New DHCP Server
```json
{
    "address-pool": "easyfi-hs-pool-<vlan_id>", // Same as the name given when creating the pool.
    "authoritative": "yes",
    "disabled": "false",
    "interface": "easyfi-vlan-<vlan_id>", // Same as the 'name' given when creating the VLAN.
    "lease-time": "30m",
    "name": "easyfi-hs-dhcp-<vlan_id>",
    "use-radius": "no"
}
```

### 8. Add a New DHCP Network
```json
{
    "address": "<hotspot_ip_subnet>",  // Refer to the general notes.
    "gateway": "100.65.0.1",  // First from the subnet. Refer to the general notes.
    "netmask": "24",  // Refer to the no. of users in the general notes.
    "dns-server": "100.65.0.1" // First from the subnet. Refer to the general notes.
}
```


### 9. Whitelist the RADIUS Server IP in the HotSpot Server
Hint: Walled-Garden IPs
```json
{
    "action": "accept",
    "dst-address": "<radius_server_ip>" // Received from the portal.
}
```

### 10. Add a New RADIUS Server:
```json
{
    "accounting-port": "1813",
    "address": "<radius_server_ip>",  // Received from the portal.
    "authentication-port": "1812",
    "disabled": "false",
    "protocol": "udp",
    "secret": "<radius_server_secret>",  // Received from the portal.
    "service": "ppp,login,hotspot,dhcp",
    "timeout": "300ms"
}
```

### 11. Allow Incoming Communication from the RADIUS Server to the MikroTik Device
```json
{
    "accept": "yes",
    "port": "3799"
}
```


### 12. Add a New DNS Server
```json
{
    "allow-remote-requests": "true",
    "servers": "8.8.8.8,8.8.4.4"
}
```


### 13. Add Firewall Rules for NAT-ing
**NOTE:** Looping needed to split the bigger IP subnet into smaller subnets. 
```json
{
    "action": "src-nat",
    "chain": "srcnat",
    "disabled": "false",
    "src-address": "100.65.0.16/28",
    "to-addresses": "111.222.111.111" // Ask the /28 public IP
}
```

### 14. Add a New SNMP Community
```json
{
    "addresses": "::/0",
    "authentication-password": "",
    "authentication-protocol": "MD5",
    "disabled": "false",
    "encryption-password": "",
    "encryption-protocol": "DES",
    "name": "<random_16_chars>",
    "read-access": "true",
    "security": "none",
    "write-access": "false" // ALWAYS FALSE
}
```


---

## Steps for PPPoE

### 1. Interface 
- Enlist the available interfaces.
- Select the first one that has field `"running"` set to `"false"`, and pick its `".id"`.
- Rename it to `"easyfi-ppp"` by its `".id"`.

### 2. Create a VLAN
Create a VLAN with the following config:
```json
{
    "name": "easyfi-vlan-<vlan_id>",
    "interface": "easyfi-ppp",  // The name that was given in the previous step.
    "vlan-id": "<vlan_id>",  // From the config received on the portal.
    "disabled": "no"
}
```

### 3. Add a New IP Pool for PPPoE Users
```json
{
    "name": "easyfi-ppp-pool-<vlan_id>",
    "ranges": "<pppoe_ip_subnet>"  // Refer to the general notes.
}
```

### 4. Add a New PPPoE Profile
```json
{
    "address-list": "",
    "bridge-learning": "default",
    "change-tcp-mss": "yes",
    "dns-server": "8.8.8.8",
    "local-address": "102.210.175.251", // nasIP (MikroTik IP)
    "name": "easyfi-ppp-profile",
    "only-one": "yes",
    "remote-address": "easyfi-ppp-pool-<vlan_id>",
    "use-compression": "default",
    "use-encryption": "default",
    "use-ipv6": "yes",
    "use-mpls": "default",
    "use-upnp": "default"
}
```


### 5. Add a PPPoE Server
```json
{
    "address-list": "",
    "bridge-learning": "default",
    "change-tcp-mss": "yes",
    "default": "false",
    "dns-server": "8.8.8.8",
    "local-address": "102.210.175.251",
    "name": "easyfi-ppp-profile",
    "only-one": "yes",
    "remote-address": "easyfi-ppp-pool-2001",
    "use-compression": "default",
    "use-encryption": "default",
    "use-ipv6": "yes",
    "use-mpls": "default",
    "use-upnp": "default"
}
```

### 6. Allowing User Authentication RADIUS Server
```json
{
    "accounting": "true",
    "interim-update": "3m",
    "use-circuit-id-in-nas-port-id": "false",
    "use-radius": "true"
}
```

### 7. Add a New RADIUS Server:
```json
{
    "accounting-port": "1813",
    "address": "<radius_server_ip>",  // Received from the portal.
    "authentication-port": "1812",
    "disabled": "false",
    "protocol": "udp",
    "secret": "<radius_server_secret>",  // Received from the portal.
    "service": "ppp,login,hotspot,dhcp",
    "timeout": "300ms"
}
```

### 8. Allow Incoming Communication from the RADIUS Server to the MikroTik Device
```json
{
    "accept": "yes",
    "port": "3799"
}
```

### 9. Add Firewall Rules for NAT-ing
**NOTE:** Looping needed to split the bigger IP subnet into smaller subnets. 
```json
{
    "action": "src-nat",
    "chain": "srcnat",
    "disabled": "false",
    "src-address": "100.64.0.16/28",
    "to-addresses": "111.222.111.111"
}
```


### 10. Add a New SNMP Community
```json
{
    "addresses": "::/0",
    "authentication-password": "",
    "authentication-protocol": "MD5",
    "disabled": "false",
    "encryption-password": "",
    "encryption-protocol": "DES",
    "name": "<random_16_chars>",
    "read-access": "true",
    "security": "none",
    "write-access": "false" // ALWAYS FALSE
}
```




































---

### General Notes: 

- Master Block Private IP series used for Active Customers PPPoE and HotSpot range is 100.64.0.0/10
- - Private IP series used for Active Customers PPPoE and is 100.64.0.0/16
- Private IP series used for Active Customers  HotSpot range is 100.65.0.0/16
- Private IP series used for Deactivated Customers PPPoE range is 10.0.0.0/16

---

### Steps for PPPoE:

- Create IP Pool.
- /ip/pool
- Add a new pool with the `"Name"` set to `"permitted"` and `Addresses` set to `100.64.0.0/24`.
- Add a new pool with the `"Name"` set to `"deactived"` and `Addresses` set to `10.0.0.0/16`.
- Create a PPPoE profile.
- /ppp/profiles
- Add a local address (Local Address is the WAN IP of the MikroTik) to the profile. 
- Add a remote address to the profile with the `Name` set to `"permitted"`.
- Add a DNS server to the profile.
- Change `TCP MSS` to `"yes"`
- Change `Limits -> Only One` to `"yes"`
- /interface/pppoe-server
- Add a new server.
- Add service name (as per req.)
- Select the interface.
- Select the profile.
- Select authentication mechanism (chap/pap/mschap1/mschap2).
- Keepalive Timeout 900
- /ppp/secret/ppp-authorization and accounting, select use radius and accounting.
- Go to RADIUS
- Add service (select: ppp, login, hotspot, dhcp)
- Put in the RADIUS server's addr in the address col, select UDP as the protocol, put the secret.
- Go to IP firewall.
- NAT
- Create source-map (as per req.)

---

### Steps for HotSpot:

- Create IP Pool.
- /ip/pool
- Add a new pool with the `"Name"` set to `"hotspot"` and `Addresses` set to `100.65.0.0/24`.
- IP -> Hotspot -> Add -> Server Name = "New hotspot" -> Interface -> Pool -> Name = "hotspot" -> Add
- IP -> Addresses -> Add -> Address -> First IP from the Hotspot IP Pool as the gateway (100.65.0.1/24)