# Nivetti NiOS MIBs

The following minimum parameters are required to be discovered to retrieve data using SNMP from Nivetti make Routers, in order to monitor them through a Network Management System (NMS).

---

## Required Minimum Parameters for SNMP Discovery

Standard SYSTEM-MIB is supported  
(Details to be configured in System PG)

### System Information

1. System Name
2. System Description
3. System Uptime
4. System Contact
5. System Location

---

## CPU Utilization

1. Current CPU Utilization  
   OID: .1.3.6.1.4.1.46634.1.2.5.1.1.1.5.1.3.0.1  
   CPU usage is displayed in tenths of a percent unit.  
   To get absolute percentage, divide the fetched value by 10.

2. Average CPU Utilization (1 min / 5 min / 15 min)  
   Currently Not Available

3. Per-Core Utilization  
   Per-core utilization is not applicable for this device

---

## Memory Utilization

### RAM

- Total Memory  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.6.1.3.0.1
- Used Memory  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.8.1.3.0.1
- Free Memory  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.7.1.3.0.1
- Memory Utilization (%)  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.9.1.3.0.1

---

### Internal Storage (Flash)

- Total Memory  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.6.1.3.0.2
- Used Memory  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.8.1.3.0.2
- Free Memory  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.7.1.3.0.2
- Memory Utilization (%)  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.9.1.3.0.2

---

### User Storage (Flash)

- Total Memory  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.6.1.3.0.3
- Used Memory  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.8.1.3.0.3
- Free Memory  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.7.1.3.0.3
- Memory Utilization (%)  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.2.1.9.1.3.0.3

---

## Interface Statistics

Standard IF-MIB is supported for both physical and virtual interfaces.

- Interface Name / Description
- Interface Type (Ethernet, Serial, Loopback, etc.)
- Interface Duplex Status
- Interface Status (Up / Down)
- Operational Status (Up / Down)
- Administrative Status (Up / Down)
- Interface IP Address
- Interface Subnet Mask
- Interface Index
- Interface Speed
- Inbound Octets
- Outbound Octets
- Inbound Unicast Packets
- Outbound Unicast Packets
- Inbound Discards
- Outbound Discards
- Inbound Errors
- Outbound Errors
- Input Queue Length
- Output Queue Length

---

## Temperature Sensors

Private MIB / OID

### Current Temperature Readings

- Air Inlet Temperature  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.3.1.5.1.3.0.1
- Air Outlet Temperature  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.3.1.5.1.3.0.2
- CPU Temperature  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.3.1.5.1.3.0.3

### Low Tolerance Thresholds

- Low Air Inlet Tolerance  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.3.1.6.1.3.0.1
- Low Air Outlet Tolerance  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.3.1.6.1.3.0.2
- Low CPU Tolerance  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.3.1.6.1.3.0.3

### High Tolerance Thresholds

- High Air Inlet Tolerance  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.3.1.7.1.3.0.1
- High Air Outlet Tolerance  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.3.1.7.1.3.0.2
- High CPU Tolerance  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.3.1.7.1.3.0.3

---

## Power Supply Status

Use: NIOS-CHASSIS-MIB  
Displayed only when the power module is ON

### Power Module A

- State  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.4.1.992.0
- Failure Reason  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.5.1.992.0
- Input Voltage  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.6.1.992.0
- Output Voltage  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.7.1.992.0
- Input Current  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.8.1.992.0
- Output Current  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.9.1.992.0

### Power Module B

- State  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.4.1.993.0
- Failure Reason  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.5.1.993.0
- Input Voltage  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.6.1.993.0
- Output Voltage  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.7.1.993.0
- Input Current  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.8.1.993.0
- Output Current  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.6.1.9.1.993.0

---

## Fan Status

Private MIB / OID

### Fan 1

- State (RPM)  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.5.1.5.1.255.0.1
- Speed (RPM)  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.5.1.6.1.255.0.1

### Fan 2

- State  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.5.1.5.1.255.0.2
- Speed (RPM)  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.5.1.6.1.255.0.2

### Fan 3

- State  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.5.1.5.1.255.0.3
- Speed (RPM)  
  OID: .1.3.6.1.4.1.46634.1.2.5.1.5.1.6.1.255.0.3

---

## Routing Table Information (Summary)

- Number of active routes
- Number of OSPF / BGP neighbors

Currently Not Available  
Please share the OIDs being used in the EMS for other devices in the network.

---

## Session Information (NAT)

- Number of active NAT sessions

Additional details required.  
Please share the OIDs currently used in the EMS for other devices.

---

## SLA Monitoring Parameters

Additional details required.  
Please share the OIDs currently used in the EMS for other devices.

- End-to-End Latency (e.g., ICMP RTT)
- Jitter
- Packet Loss
- SLA Operation Status (Active / Failed)
- SLA Threshold Breach Status
